### LHPP — PECS/POGANY

#### LHPP AD 2.1 AERODROME LOCATION INDICATOR AND NAME

LHPP — PECS/POGANY

#### LHPP AD 2.2 AERODROME GEOGRAPHICAL AND ADMINISTRATIVE DATA

1 | ARP coordinates and site at AD | 455921N 0181432E,at the geometrical centre of the RWY
2 | Direction and distance from (city) | 9 KM SSE from the centre of Pécs
3 | Elevation/Reference temperature | 198 M / 27.4°C
4 | MAG VAR/ annual change | 5° E (2024) / 0.1° increasing
5 | AD Administration, address, telephone, telefax, AFS | Post: Pecs/Poganyi Repuloteret Mukodteto Kft. H-7666 Pogany, Repuloter 08/9 Tel:(+36) 72-526-140 AFS:LHPPZPZX SITA:PEVOPXH Email:info@airportpecs.hu; fly@airportpecs.hu URL:www.airportpecs.hu
6 | Types of traffic permitted (IFR/VFR) | IFR-VFR
7 | Remarks | Nil

#### LHPP AD 2.3 OPERATIONAL HOURS

1 | AD Administration | MAY 01 - AUG 31 MON, TUE, WED, THU, FRI: 0800 - 1800 (0700-1700) SAT, SUN, Legal Holiday: 0900 - 1700 (0800-1600) MAR 01 - APR 30, SEP 01 - OCT 31 MON, TUE, WED, THU, FRI: 0800 - 1600 (0700-1500) SAT, SUN, Legal Holiday: 0900 - 1500 (0800-1400) NOV 01 - FEB 28 MON, TUE, WED, THU, FRI: 0800 - 1400 SAT, SUN, Legal Holiday: 0900 - 1300 (PPR 0500 - 2100)
2 | Customs and immigration | 3 workdays prior request required for flights outside the Schengen Region departing/arriving to/from LHPP. Further information: Tel:(+36) 72-526-156 Email:info@airportpecs.hu
3 | Health and sanitation | Nil
4 | AIS Briefing Office | Nil
5 | ATS Reporting Office (ARO) | Nil
6 | MET Briefing Office | H24
7 | ATS | AFIS JAN-FEB: 0800-1400 (0700-1300) MAR: 0800-1600 (0700-1500) APR-SEP: 0730-SS-30 (0630-SS-30) OCT: 0800-1600 (0700-1500) NOV-DEC: 0800-1400 (0700-1300)
8 | Fuelling | As Administration
9 | Handling | As Administration
10 | Security | H24
11 | De-icing | As Administration
12 | Remarks | Nil

#### LHPP AD 2.4 HANDLING SERVICES AND FACILITIES

1 | Cargo-handling facilities | Nil
2 | Fuel/oil types | AVGAS 100LL, JET-A1, Gasoline 95
3 | Fuelling facilities/capacity | Available (10000 L)
4 | De-icing facilities | Available at parking stands on request
5 | Hangar space for visiting aircraft | up to 20 M wingspan on request
6 | Repair facilities for visiting aircraft | Nil
7 | Remarks | GPU

#### LHPP AD 2.5 PASSENGER FACILITIES

1 | Hotels | In the city
2 | Restaurants in the city | In the city
3 | Transportation | Taxi, local public coach, car hire
4 | Medical facilities | First aid at AD, hospital in the city.
5 | Bank and Post Office | In the city, credit card acceptance at AD
6 | Tourist Office | In the city
7 | Remarks | Accomodation for limited number of guest in Pogany

#### LHPP AD 2.6 RESCUE AND FIRE FIGHTING SERVICES

1 | AD category for fire fighting | A3
2 | Rescue equipment | 1 fire truck and hand operated fire extinguishers
3 | Capability for removal of disabled aircraft | Available (restricted, up to 30 tons)
4 | Remarks | For CAT A5, 3 hours prior request required.

#### LHPP AD 2.7 Runway surface condition assessment and reporting, and snow plan

1 | Types of clearing equipment | 1 snow plough and sweeper, 1 carbamid spreader
2 | Clearance priorities | RWY, TWYs, Apron 1, Apron 2
3 | Use of material for movement area surface treatment | Nil
4 | Specially prepared winter runways | Nil
5 | Remarks | Nil

#### LHPP AD 2.8 APRONS, TAXIWAYS AND CHECK LOCATIONS/POSITIONS DATA

1 | Apron surface and strength | Surface: | CONC
Strength: | Apron 1: 35/R/B/W/T Apron 2: 37/R/B/W/T
2 | Taxiway width, surface and strength | Width: | TWY A: 15 M TWY A1: 10 M
Surface: | asphalt
Strength: | TWY A and A1: 37/F/C/W/T
3 | Altimeter checkpoint location and elevation | Location: | Nil
Elevation: |
4 | VOR checkpoints | Nil
5 | INS checkpoints | Nil
6 | Remarks | Turning bay at treshold RWY 33. (43.30 M X 8.54 M)

#### LHPP AD 2.9 SURFACE MOVEMENT GUIDANCE AND CONTROL SYSTEM AND MARKINGS

1 | Use of aircraft stand ID signs, TWY guide lines and visual docking/parking guidance system of aircraft stands | TWY centre lines, guide lines on apron. Centrelines, holding point marking.
2 | RWY and TWY markings and LGT | RWY: designator, threshold, TDZ, centre line markings TWYs: centre lines, holding point marking
3 | Stop bars | Nil
4 | Remarks | Nil

#### LHPP AD 2.10 AERODROME OBSTACLES

Data for Area 2 and Area 3 See GEN 3.1

#### LHPP AD 2.11 METEOROLOGICAL INFORMATION PROVIDED

1 | Associated MET Office | Hungarian Meteorological Service (HMS) Unit of Aviation Meteorology
2 | Hours of service | H24
3 | Office responsible for TAF preparation Periods of validity | Hungarian Meteorological Service (HMS) Unit of Aviation Meteorology Periods of validity: 9 HRs, Interval of issuance: 3 HRs in operational hours of aerodrome
4 | Type of landing forecast Interval of issuance | Nil
5 | Briefing/consultation provided | Written briefing: https://aviation.met.hu Consultation via phone: +36-90-603-421 Consultation via e-mail: rvo@met.hu (HMS) See GEN 3.5
6 | Flight documentation Language(s) used | Charts, abbreviated plain language text Hungarian, English
7 | Charts and other information available for briefing or consultation | Charts, aerodrome reports and forecasts in EUR region, area forecasts, MET. observations and warnings in Budapest FIR
8 | Supplementary equipment available for providing information | Telephone/Telefax
9 | ATS Units provided with information | Budapest FIC (on request); AFIS (on request)
10 | Additional information | Nil

#### LHPP AD 2.12 RUNWAY PHYSICAL CHARACTERISTICS

Designations RWY NR | TRUE BRG | Dimensions of RWY (M) | Strength (PCN) and surface of RWY and SWY | THR coordinates RWY end coordinates THR geoid undulation | THR elevation and highest elevation of TDZ of precision APP RWY
--- | --- | --- | --- | --- | ---
1 | 2 | 3 | 4 | 5 | 6
15 | 157.53° GEO | 1500 x 30 | 38/F/B/W/T ASPH | 455943.62N 0181418.32E 455858.74N 0181444.95E 44.7 M | 198 M
33 | 337.53° GEO | 1500 x 30 | 38/F/B/W/T ASPH | 455858.74N 0181444.95E 455943.62N 0181418.32E 44.7 M | 195.1 M

Designations RWY NR | Slope of RWY - SWY | SWY dimensions (M) | CWY dimensions (M) | Strip dimensions (M) | RESA dimensions (M) surface | Location of arresting system | OFZ | Remarks
--- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 7 | 8 | 9 | 10 | 11 | 12 | 13 | 14
15 | -0.10%/-0.87% | Nil | Nil | 1620 x 300 | 360 x 90 grass | Nil | Nil | Nil
33 | +0.87%/+0.10% | Nil | Nil | 1620 x 300 | 360 x 90 grass | Nil | Nil | Nil

#### LHPP AD 2.13 DECLARED DISTANCES

RWY Designator | TORA (M) | TODA (M) | ASDA (M) | LDA (M) | Remarks
--- | --- | --- | --- | --- | ---
1 | 2 | 3 | 4 | 5 | 6
15 | 1500 | 1500 | 1500 | 1500 | Nil
33 | 1500 | 1500 | 1500 | 1500 | Nil

#### LHPP AD 2.14 APPROACH AND RUNWAY LIGHTING

RWY Designator | APCH LGT type LEN INTST | THR LGT colour WBAR | VASIS (MEHT) | TDZ LGT LEN | RWY Centre Line LGT Length, spacing, colour, INTST | RWY edge LGT LEN, spacing colour INTST | RWY End LGT colour WBAR | SWY LGT LEN (M) colour | Remarks
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 2 | 3 | 4 | 5 | 6 | 7 | 8 | 9 | 10
15 | SALS 420 M LIM | Green | 3.36° (15 M) | Nil | Nil | 1500 M 60 M White/Yellow LIH | RED | Nil | Nil
33 | CAT1 barrette 900 M LIH | Green | 3° (17 M) | Nil | Nil | 1500 M 60 M White/Yellow LIH | RED | Nil | Nil

#### LHPP AD 2.15 OTHER LIGHTING AND SECONDARY POWER SUPPLY

1 | ABN/IBN location, characteristics and hours of operation | Nil
2 | LDI location and LGT Anemometer location and LGT | Nil
3 | TWY edge and centre line lighting | TWY edge lighting on TWY A, in 102 M length
4 | Secondary power supply | GPU diesel ground power unit (152 kW, 10-hour operating time)
5 | Remarks | Retroreflective edge markers on the other section of TWY A and Aprons

#### LHPP AD 2.16 HELICOPTER LANDING AREA

NIL

#### LHPP AD 2.17 AIR TRAFFIC SERVICES AIRSPACE

1 | Designation and lateral limits | PECS-POGANY TIZ 454614N 0181508E - 455106N 0182820E - 461304N 0182154E - 461402N 0181906E - 460854N 0180424E - 455347N 0175950E - 454614N 0181508E
2 | Vertical limits | 9500 FT ALT GND
3 | Airspace classification | G
4 | ATS unit call sign Language(s) | Pogány Info EN, HU
5 | Transition altitude | 10000 FT AMSL
6 | Hours of applicability | As ATS Administration
7 | Remarks | Air Traffic Advisory Service is not AVBL in the class G airspace LHPP TIZ.

#### LHPP AD 2.18 AIR TRAFFIC SERVICES COMMUNICATION FACILITIES

Service designation | Call sign | Channel(s) | SATVOICE number(s) | Logon Address | Hours of operation | Remarks
--- | --- | --- | --- | --- | --- | ---
1 | 2 | 3 | 4 | 5 | 6 | 7
AFIS | Pogány Info | 126.915 CH | Nil | Nil | As ATS Administration | Nil

#### LHPP AD 2.19 RADIO NAVIGATION AND LANDING AIDS

MAG VAR Type of supported OPS (for VOR/ILS/MLS, give declination) | ID | Frequency(ies) | Hours of operation | Position of transmitting antenna coordinates | Elevation of DME transmitting antenna | Remarks
--- | --- | --- | --- | --- | --- | ---
1 | 2 | 3 | 4 | 5 | 6 | 7
L | PP | 412 KHZ | H24 | 460021.0N 0181358.0E |  | Nil
ILS 33 (CAT I) |
LLZ | PCS | 108.35 MHZ | H24 | 455952.2N 0181413.3E |  |
GP |  | 333.95 MHZ | H24 | 455905.3N 0181434.9E |  | GP angle: 3
DME | PCS | 20Y | H24 | 455905.3N 0181434.9E | 196 M |

#### LHPP AD 2.20 LOCAL AERODROME REGULATIONS

The village of Pogány must be avoided by all engine propelled aircraft, except aircraft making instrument approach for RWY 33.

Local training flights outside opening hours allowed only for contracted partners or on 24 hours prior request.

#### LHPP AD 2.21 NOISE ABATEMENT PROCEDURES

NIL

#### LHPP AD 2.22 FLIGHT PROCEDURES

See attached instrument approach chart.

#### LHPP AD 2.23 ADDITIONAL INFORMATION

NIL

#### LHPP AD 2.24 CHARTS RELATED TO THE AERODROME

AD_2-LHPP-ADC | AERODROME CHART - ICAO
../graphics/eAIP/LH_AD_2_LHPP_ADC_en.pdf
AD_2-LHPP-AOCA-1533 | AERODROME OBSTACLE CHART - ICAO TYPE A OPERATING LIMITATIONS
../graphics/eAIP/LH_AD_2_LHPP_AOCA_1533_en.pdf
AD_2-LHPP-ILS-LOC-33 | INSTRUMENT APPROACH CHART - ICAO
../graphics/eAIP/LH_AD_2_LHPP_ILS_OR_LOC_33_en.pdf
AD_2-LHPP-NDB-15 | INSTRUMENT APPROACH CHART - ICAO
../graphics/eAIP/LH_AD_2_LHPP_NDB_15_en.pdf
AD_2-LHPP-RNP_15 | INSTRUMENT APPROACH CHART - ICAO
../graphics/eAIP/LH_AD_2_LHPP_RNP_15_en.pdf
AD_2-LHPP-RNP_33 | INSTRUMENT APPROACH CHART - ICAO
../graphics/eAIP/LH_AD_2_LHPP_RNP_33_en.pdf
AD_2-LHPP-VAC | VISUAL APPROACH CHART - ICAO
../graphics/eAIP/LH_AD_2_LHPP_VAC_en.pdf

#### LHPP AD 2.25 VISUAL SEGMENT SURFACE (VSS) PENETRATION

RWY15
Obstacle penetrating VSS | Affected procedures | Affected OCA/H
LHPP_AREA2B_P_036 | AD 2-LHPP-NDB-15, AD 2-LHPP-RNP-15 (except LPV minima) | NIL
LHPP_AREA2B_P_035 | AD 2-LHPP-NDB-15, AD 2-LHPP-RNP-15 (except LPV minima) | NIL

RWY33
Obstacle penetrating VSS | Affected procedures | Affected OCA/H
Not applicable